CMT727 and HM 80 binding procedure:



1. Press both buttons at the HM 80 (approx. 4 s) until LED 4 (“!”)

flashes evenly steadily.

2. Press the **OFF** button on the room thermostat. Then press the  and  buttons together along with the  button. The unit will display InSt and ‘CONTROL BINDING’.

**3.** Press the green  button to send the binding signal out to the relay box. The red LED is switched off to confirm successful binding operation. If the red LED still flashes push the button again until binding is successful.

*If teaching-in is successful, LED 4 (“!”) at the HM 80*

*extinguishes.*

“I” - After 3 minutes a time-out is carried out at the

HM 80. The device is no longer in teach-in mode.

For system programming please use “CMT727 user manual” and “CMT727 installer manual”.

1)HM80 abas pogas piespiež 15 sek un izdzēšam visu lieko ja bijusi instalācija un lampiņa mirgo nevienmērīgi.

2) HM80 abas pogas spiežam 4 sekundes līdz lampiņa mirgo vienmērīgi 50/50. HM ir gatavs saņemt signālu.

3) Uz vadības pults pispiežam off (izslēgšanas pogu) un tad vienlaicīgi temperatūra uz augšu un leju un butiņa pa kreisi. Parādas INST CO

4) Piespiežamo zaļo OK pogu un lampiņai uz HM80 ir jāizdziest. Procedūra pabeigta. Piespiežot Off pogu nonākam sākotnējā pozīcijā